0
<Name>Standard
<Check>1
<ZERO>Exit
<Cut>
RDBench|180|END Batter|Accept Intercept|||0|END Batter|Intercept|0.5||Intercept Using Face||0|50|0||0|0|0|0|0|0|0|0|||END Batter|0|\G#@0.5|5|0|TW|1|N|\#@2|-0.1|0|BW|1|N|\#@
<Fill>
<Name>Sleeper Wall 0.2m if Depth >0.5m
<Check>0
<ZERO>Exit
<Cut>
RDCheckSUrface|20|Grade at 1:2 to Surface||0|0||0.5|0|
RDLabel|Check for sleeper wall|120||
RDCheckSUrface|40|Sleeper Wall||0|0||1000|0.3|
RDWidthSlope|Back of wall|BW|0|0|0.1|160|1|1|
RDLabel|Grade at 1:2 to Surface|0||
RDBatter|80|END Batter||0|0|End batter conditions for cut <1m|BAT|4|0|50|0|1|
RDLabel|Sleeper Wall|60||
RDWidthSlope||Wall|0|0.2|0.02|100|1|0|
RDGoTo|140||Check for sleeper wall|
<Fill>
RDCheckSUrface|200|Depth less than 1m||0|0||1|0|
RDLabel|Depth less than 1m|240||
RDBatter|260|END Batter||0|0||BAT|4|0|4|0||
RDCheckSUrface|360|Depth greater than 1m||0|0||1000|0|
RDLabel|Depth greater than 1m|280||
RDWidthSlope||TW|10|0|1|320|0||
<Name>Change Batter Slopes if Depth >1
<Check>1
<ZERO>Exit
<Cut>
RDCheckSUrface|580|||0|0||1|0|
RDCheckSUrface|600|Depth >1||0|0||1000|1|
RDLabel|Depth <1|620||
RDBatter|660|END Batter||0|0||BAT|4|0|6|0|0|
RDLabel|Depth >1|640|If the width of the <1m depth batter exceeds 6m then it doesn't create and ends up here|
RDWidthSlope||VERGE|5|0|1|700|0|0|
RDBatter|680|END Batter||0|0||BAT|2|0|20|0|0|
<Fill>
<Name>Batter to Rock Surface at 1:.5 then Batter at 1:3
<Check>
<ZERO>Exit
<Cut>
RDDefaults|0\G#@0|0\#@0|0\#@0|0\#@0|0\#@0|0\#@\G#@0|0\#@0|0\#@0|0\#@0|0\#@0|0\#@\G#@101.3|2\#@0|0\#@0|0\#@0|0\#@0|0\#@\G#@
RDBatter|380|Next Line|Surface1|0|0|Surface 1 is the Rock Surface - select it when applying this template|BAT|0.5|0|10|0||
RDBatter|420|END Batter||0|0|Final Batter to surface|BAT|3|0|20|0||
<Fill>
RDCheckSUrface|440|Depth <1||0|0||1|0|
RDCheckSUrface|460|Depth > 1m||0|0||1000|1|
RDLabel|Depth <1|480|Create a 1:2 batter only|
RDBatter|520|END Batter||0|0||BAT|2|0|10000|0||
RDLabel|Depth > 1m|500|Do a verge and then a steep batter|
RDWidthSlope||VERGE|10|0|1|540|0||
RDBatter|560|END Batter||0|0||BAT|0.1|0|10|0||
<Name>Bench 5m high with 2m bench
<Check>1
<ZERO>Exit
<Cut>
RDBench|180|END Batter|Accept Intercept|||0|END Batter|Intercept|0.5||Intercept Using Face||0|50|0||0|0|0|0|0|0|0|0|||END Batter|0|\G#@0.5|5|0|TW|1|N|\#@2|-0.1|0|BW|1|N|\#@
<Fill>
<Name>1:3 batter to alternate surface
<Check>1
<ZERO>Exit
<Cut>
RDDefaults|0\G#@0|0\#@0|0\#@0|0\#@0|0\#@0|0\#@\G#@0|0\#@0|0\#@0|0\#@0|0\#@0|0\#@\G#@100.5|0\#@100|0\#@100|0\#@100|0\#@100|0\#@\G#@
RDBatter|20|END Batter|Surface1|0|0|SET TO MATCH TO SURFACE1|BAT|3|0|100|0|1|
<Fill>
